{"text_format":"1","workbook":"xlsx","n_sheets":19,"sheets":["About","TC","EN","SC","DBM","DB","TM_S","TM_D","Sheet2","TM_S-bp","LSI","Sheet1","DB_LSI","DB_METAL","DB_PCB","DB_TIM","DB_DRV","DB_HS","HS_D"],"not_rendered":{"charts":12,"images":122,"macros":1,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"About","index":0,"n_rows":31,"n_cols":11,"rows_kept":31,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Thermal Analysis Module",null,"(with HeatSink Design)"]
[null,null,null,null,null,null,null,null,"熱學分析模組",null,"(帶散熱器設計)"]
[null,null,null,null,null,null,null,null,"热分析模组",null,"(带散热器设计)"]
[null,null,null,null,null,null,null,null,"PROGCODE",120]
[null,null,null,null,null,null,null,null,"VER",20]
[null,null,null,null,null,null,null,null,"FUNC",-1]
[null,null,null,null,null,null,null,null,"CODE"]
[null,null,null,null,null,null,null,null,"MAC","28:18:78:D2:C4:47"]
[null,null,null,null,null,null,null,null,"Purchasing #","A0016"]
[null,null,null,null,null,null,null,null,"Computer+User","CADMUSSURFACE-Cadmus Yuan"]
[null,null,null,null,null,null,null,null,"(Please return MAC address for more functions)"]
[null,null,null,null,null,null,null,null,"(請回傳MAC地址以獲得更高權限)"]
[]
[]
[null,null,null,null,null,null,null,null,"Email: sales@ichijouriki.com"]
[null,null,null,null,null,null,null,null,"www.ichijouriki.com"]
[null,null,null,null,null,null,null,null,"https://www.facebook.com/ichijouriki"]

{"sheet":"TC","index":1,"n_rows":38,"n_cols":34,"rows_kept":38,"cut":false,"hidden":true,"merged":[]}
[null,null,"快速熱分析工具(TAM)",null,null,null,null,null,null,null,"等效Rth","Tj","Tj","等效Rth"]
[null,null,"環境溫度",null,null,null,null,null,"Rth","效率",null,null,null,null,null,null,null,"Rth","效率",null,"環境溫度"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"材料",null,null,null,null,"光源個數","電流(mA)",null,null,"總功率",null,"幫助檔案："]
[null,null,"光源",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"光源"]
[null,null,null,null,null,null,"面積","厚度","總功率",null,null,null,null,null,"k","面積","厚度",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"線上幫助：","IJR website"]
[null,null,null,"材料",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"封裝形式：",null,null,"PCB 面積",null,null,"Email: ","sales@ichijouriki.com"]
[null,null,"焊點",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"焊點"]
[null,null,"焊點",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"焊點",null,null,null,null,null,null,null,null,null,null,"(1)","LED"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(2)","焊點"]
[null,null,"PCB",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PCB",null,null,null,null,null,null,null,null,null,null,"(3)","PCB"]
[null,null,"熱介材料",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"熱介材料",null,null,null,null,null,null,null,null,null,null,"(4)","熱介材料"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(5)","散熱器"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(6)","鰭片"]
[null,null,null,"材料","幾何尺寸",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"材料","幾何尺寸",null,null,null,null,null,null,null,null,"(7)","環境溫度"]
[null,null,"散熱器1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"散熱器1"]
[null,null,"散熱器2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"散熱器2"]
[null,null,"Driver",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Driver"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Temp1",null,null,null,"Temp1"]
[null,null,null,null,null,"solder","1/r","1/r",null,null,null,"Rth1",33.16123771736995,null,null,"Rth1",241.26713927015109,null,null,null,"solder","1/r","1/r"]
[null,null,null,null,null,null,0,0,null,null,"LS",0.17,32.529408152736963,null,"LS",0.27500000000000002,233.92872090673782,null,null,null,null,2.7272428571428571,0.90281142857142849]
[null,null,null,null,null,"sum 1/r",0,0,null,null,"SOLDER",0,32.529408152736963,null,"SOLDER",6.8869493490455484E-3,233.74494157738897,null,null,null,"sum 1/r",3.6300542857142855,0.27547797396182194]
[null,null,null,null,null,null,null,null,null,null,"PCB",3.7037037037037038E-3,32.515642802744956,null,"PCB",1.1600000000000001E-2,233.43539374824135]
[null,null,null,null,null,null,"Rth","Q",null,null,"TIM",0.26041666666666669,31.547766631432165,null,"TIM",6.6666666666666662E-3,233.25749269700708,null,null,null,"Rth","Q"]
[null,null,null,null,null,"HS1",0.89977473243603989,1.1601376139602646,null,null,"HS",0.89977473243603989,28.203623822827293,null,"HS",3.4867631181451126,140.21266907857711,null,null,"HS1",3.4867631181451126,0.29580277313262821]
[null,null,null,null,null,"HS2",2125.2440430763663,5.1631814350465671E-4,null,null,"ENV",null,25,null,"ENV",null,50,null,null,"HS2",1525.4490490675551,7.479272152569851E-4]
[null,null,null,null,null,null,0.89977473243603989,1.1601376139602646,null,null,null,1.3338951028064103,null,null,null,3.7869167341608247,null,null,null,null,3.4867631181451126,0.29580277313262821]
[null,null,null,null,null,null,null,null,null,null,"Heat",3.7166444978411173,1.1601376139602646,null,null,26.685157685139202,0.29580277313262821]

{"sheet":"EN","index":2,"n_rows":38,"n_cols":34,"rows_kept":38,"cut":false,"hidden":true,"merged":[]}
[null,null,"Thermal Analysis Module (TAM)",null,null,null,null,null,null,null,"Eq. Rth","Tj","Tj","Eq. Rth"]
[null,null,"Env Temp",null,null,null,null,null,"Rth","Efficiency",null,null,null,null,null,null,null,"Rth","Efficiency",null,"Env Temp",50,"( C)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Material",null,null,null,null,"# of LS","Current (mA)",null,null,"Total P",null,"Help File"]
[null,null,"L.S. ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LightSource"]
[null,null,null,null,null,null,"Area","Thickness","Total P",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Online Help","IJR website"]
[null,null,null,"Material",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Form:",null,null,"PCB Area",null,null,"Email: ","sales@ichijouriki.com"]
[null,null,"Solder J.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solder Joint"]
[null,null,"Solder J.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solder Joint",null,null,null,null,null,null,null,null,null,null,1,"LED"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"Solder"]
[null,null,"PCB",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PCB",null,null,null,null,null,null,null,null,null,null,3,"PCB"]
[null,null,"TIM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TIM",null,null,null,null,null,null,null,null,null,null,4,"TIM"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"HS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"Fin"]
[null,null,null,"Material","Geometry",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Material","Geometry",null,null,null,null,null,null,null,null,7,"Env Temp"]
[null,null,"HS1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HS1"]
[null,null,"HS2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"HS2"]
[null,null,"Driver",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Driver"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Temp1",null,null,null,"Temp1"]
[null,null,null,null,null,"solder","1/r","1/r",null,null,null,"Rth1",37.118964681739946,null,null,"Rth1",241.26713927015109,null,null,null,"solder","1/r","1/r"]
[null,null,null,null,null,null,3.2915000000000006E-5,0.90281142857142849,null,null,"LS",11,29.780546318326667,null,"LS",0.27500000000000002,233.92872090673782,null,null,null,null,2.7272428571428571,0.90281142857142849]
[null,null,null,null,null,"sum 1/r",0.90284434357142851,1.1076106386669575,null,null,"SOLDER",1.1076106386669575,29.041627204662529,null,"SOLDER",6.8869493490455484E-3,233.74494157738897,null,null,null,"sum 1/r",3.6300542857142855,0.27547797396182194]
[null,null,null,null,null,null,null,null,null,null,"PCB",3.2615786040443577,26.865733720877532,null,"PCB",1.1600000000000001E-2,233.43539374824135]
[null,null,null,null,null,null,"Rth","Q",null,null,"TIM",0.66666666666666674,26.42098109279188,null,"TIM",6.6666666666666662E-3,233.25749269700708,null,null,null,"Rth","Q"]
[null,null,null,null,null,"HS1",1.0708553665790255,0.944162863321239,null,null,"HS",1.0708553665790255,25.706582484913408,null,"HS",3.4867631181451126,140.21266907857711,null,null,"HS1",3.4867631181451126,0.29580277313262821]
[null,null,null,null,null,"HS2",2125.2440430763663,5.1631814350465671E-4,null,null,"ENV",null,25,null,"ENV",null,50,null,null,"HS2",1525.4490490675551,7.479272152569851E-4]
[null,null,null,null,null,null,1.0708553665790255,0.944162863321239,null,null,null,17.106711275957007,null,null,null,3.7869167341608247,null,null,null,null,3.4867631181451126,0.29580277313262821]
[null,null,null,null,null,null,null,null,null,null,"Heat",0.66712894212848006,0.944162863321239,null,null,26.685157685139202,0.29580277313262821]

{"sheet":"SC","index":3,"n_rows":17,"n_cols":34,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
[null,null,"快速热分析工具(TAM)",null,null,null,null,null,null,null,"等效Rth","Tj","Tj","等效Rth"]
[null,null,"环境温度",null,null,null,null,null,null,"效率",null,null,null,null,null,null,null,null,"效率",null,"环境温度",50,"( C)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"材料",null,null,null,null,"光源个数","电流(mA)",null,null,"总功率",null,"帮助档案："]
[null,null,"光源",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"光源"]
[null,null,null,null,null,null,"面积","厚度","总功率",null,null,null,null,null,null,"面积","厚度",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"线上帮助：","IJR website"]
[null,null,null,"材料",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"封装形式：",null,null,"PCB 面积",null,null,"Email: ","sales@ichijouriki.com"]
[null,null,"焊点",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"焊点"]
[null,null,"焊点",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"焊点",null,null,null,null,null,null,null,null,null,null,1,"LED"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,"焊点"]
[null,null,"PCB",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PCB",null,null,null,null,null,null,null,null,null,null,3,"PCB"]
[null,null,"热介材料",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"热介材料",null,null,null,null,null,null,null,null,null,null,4,"热介材料"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"散热器"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,"鳍片"]
[null,null,null,"材料","几何尺寸",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"材料","几何尺寸",null,null,null,null,null,null,null,null,7,"环境温度"]
[null,null,"散热器1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"散热器1"]
[null,null,"散热器2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"散热器2"]
[null,null,"Driver",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Driver"]

{"sheet":"DBM","index":4,"n_rows":8,"n_cols":10,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
[]
[null,"資料庫管理",null,"Database management"]
[null,"数据库管理"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,"Number of data",null,97]

{"sheet":"DB","index":5,"n_rows":15,"n_cols":8,"rows_kept":15,"cut":false,"hidden":false,"merged":[[13,4,13,5],[14,4,14,5],[8,2,8,3],[8,4,8,5],[9,4,9,5],[10,4,10,5],[11,4,11,5],[12,4,12,5]]}
[]
[]
[null,null,null,null,null,"Thermal Analysis Module",null,"(with HeatSink Design)"]
[null,null,null,null,null,"熱學分析模組",null,"(帶散熱器設計)"]
[null,null,null,null,null,"热分析模组",null,"(带散热器设计)"]
[]
[]
[]
[null,null,"Database / 現有資料庫",null,"Number of data / 資料個數"]
[null,null,"LightSource","光源",97]
[null,null,"Metal","金屬",10]
[null,null,"PCB","電路板",10]
[null,null,"TIM","熱介面材料",5]
[null,null,"Driver","驅動",2]
[null,null,"HeatSink","散熱器",32]

{"sheet":"TM_S","index":6,"n_rows":38,"n_cols":35,"rows_kept":38,"cut":false,"hidden":false,"merged":[]}
[null,null,"快速热分析工具(TAM)",null,null,null,null,null,null,null,"等效Rth","Tj","Tj","等效Rth"]
[null,null,"环境温度",25,"  (C)","n","If","Vf","Rth","效率",{"$f":"+L37","v":0.19349749601440619},{"$f":"+M35+L37*L38","v":42.887427988121559},{"$f":"+Q35+P37*P38","v":76.879869532658574},{"$f":"+P37","v":12.00609756097561},"n","If","Vf","Rth","效率",null,"环境温度",50,"( C)"]
[null,null,null,null,null,null,"(mA)","(V)","(C/W)","%",null,null,null,null,null,"(mA)","(V)","(C/W)","%",null,null,"材料",null,null,null,null,"光源个数","电流(mA)",null,null,"总功率",null,"帮助档案：","幫助檔案："]
[null,null,"光源","Nichia-NF2L757GT",null,{"$f":"+AA4","v":255},{"$f":"+AB4","v":180},3.0192779643124998,11,50,null,null,null,null,1,20,6.6712894212848006,11,50,null,"光源",null,null,null,null,null,255,180,null,null,{"$f":"+I6","v":138.58485856194375},"W"]
[null,null,null,null,null,"k","面积","厚度","总功率",null,null,null,null,null,"k","面积","厚度",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"线上帮助：","IJR website","IJR website"]
[null,null,null,"材料",null,"(W/mK)","(mm2)","(mm)",{"$f":"H4*G4*F4/1000","v":138.58485856194375},null,null,null,null,null,"(W/mK)","(mm2)","(mm)",null,null,null,null,null,null,null,null,null,"封装形式：",null,null,"PCB 面积",{"$f":"250*300","v":75000},"mm2","Email: ","sales@ichijouriki.com","sales@ichijouriki.com"]
[null,null,"焊点","SAC-G",null,58,3.2915000000000001,0.15,null,null,null,null,null,null,0,3.2915000000000001,7.0000000000000007E-2,null,null,null,"焊点"]
[null,null,"焊点","SAC-G",null,58,1.0895999999999999,0.15,null,null,null,null,null,null,0,1.0895999999999999,7.0000000000000007E-2,null,null,null,"焊点",null,null,null,null,null,null,null,null,null,42.887427988121559,"1","LED"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(a*b)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,39.898342803452181,"2","焊点"]
[null,null,"PCB","Ideal-FR4-G",null,0.2,{"$f":"IF(AE6>0,AE6/F4,H20*J15/F4)","v":294.11764705882354},1.2,null,null,null,null,null,null,0,500,0.11600000000000001,null,null,null,"PCB",null,null,null,null,null,null,null,null,null,39.737934920853739,"3","PCB"]
[null,null,"热介材料","Eporite-TIM1101",null,2,{"$f":"+G10","v":294.11764705882354},0.5,null,null,null,null,null,null,0,500,0.2,null,null,null,"热介材料",null,null,null,null,null,null,null,null,null,34.194540578375992,"4","热介材料"]
[null,null,null,null,null,"Thermal",null,"Fin",null,null,null,null,null,null,"Thermal",null,"Fin",null,null,null,null,null,null,null,null,null,null,null,null,null,33.963565814106083,"5","散热器"]
[null,null,null,null,null,"h","k","n","b","t",null,null,null,null,"h","k","n","b","t",null,null,null,null,null,null,null,null,null,null,null,29.479516429498183,"6","鳍片"]
[null,null,null,"材料","几何尺寸","(W/m2K)","(W/mK)",null,"(mm)","(mm)",null,null,null,null,"(W/m2K)","(W/mK)",null,"(mm)","(mm)",null,null,"材料","几何尺寸",null,null,null,null,null,null,null,25,"7","环境温度"]
[null,null,"散热器1","Al-6063-Extruded","PCC-Hproject-600W",8,170,32,1,300,null,null,null,null,100,164,0,1E-3,100,null,"散热器1","Al-G","G-P100x100x10-7W"]
[null,null,"散热器2",null,null,0,0,0,5,50,null,null,null,null,0,0,15,2,90,null,"散热器2"]
[null,null,"Driver",null,0,"(W)",null,"Block",null,null,null,null,null,null,null,null,"Block",null,null,null,"Driver","DRV-Test1",2,"(W)"]
[null,null,null,null,"(W)",null,null,"L","l","delta",null,null,null,null,null,null,"L","l","delta",null,null,null,"(W)"]
[null,null,null,null,null,null,null,"(mm)","(mm)","(mm)",null,null,null,null,null,null,"(mm)","(mm)","(mm)"]
[null,null,null,null,null,null,null,300,175,1,null,null,null,null,null,null,100,1E-3,10]
[null,null,null,null,null,null,null,50,10,3,null,null,null,null,null,null,59,38,10]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Temp1",null,null,null,"Temp1"]
[null,null,null,null,null,"solder","1/r","1/r",null,null,null,"Rth1",{"$f":"+M31+L31*L38","v":42.887427988121559},null,null,"Rth1",{"$f":"+Q31+P31*P38","v":76.879869532658574},null,null,null,"solder","1/r","1/r"]
[null,null,null,null,null,null,{"$f":"+F7*G7/1000/H7","v":1.2727133333333336},{"$f":"+F8*G8/1000/H8","v":0.42131200000000002},null,null,"LS",{"$f":"I4/F4","v":4.3137254901960784E-2},{"$f":"+M32+L32*L38","v":39.898342803452181},null,"LS",{"$f":"R4/O4","v":11},{"$f":"+Q32+P32*P38","v":54.14602769631724},null,null,null,null,{"$f":"+O7*P7/1000/Q7","v":0},{"$f":"+O8*P8/1000/Q8","v":0}]
[null,null,null,null,null,"sum 1/r",{"$f":"+G31+H31","v":1.6940253333333337},{"$f":"IF(G32>0,1/G32,0)","v":0.59030994420390392},null,null,"SOLDER",{"$f":"+H32/F4","v":2.3149409576623684E-3},{"$f":"+M33+L33*L38","v":39.737934920853739},null,"SOLDER",{"$f":"+W32/O4","v":0},{"$f":"+Q33+P33*P38","v":54.14602769631724},null,null,null,"sum 1/r",{"$f":"+V31+W31","v":0},{"$f":"IF(V32>0,1/V32,0)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"PCB",{"$f":"IF(AND(F10>0,G10>0),H10/(F10*G10*0.001),0)/F4","v":7.9999999999999988E-2},{"$f":"+M34+L34*L38","v":34.194540578375992},null,"PCB",{"$f":"IF(AND(O10>0,P10>0),Q10/(O10*P10*0.001),0)/O4","v":0},{"$f":"+Q34+P34*P38","v":54.14602769631724}]
[null,null,null,null,null,null,"Rth","Q",null,null,"TIM",{"$f":"IF(AND(F11>0,G11>0),H11/(F11*G11*0.001),0)/F4","v":3.3333333333333331E-3},{"$f":"+M35+L35*L38","v":33.963565814106083},null,"TIM",{"$f":"IF(AND(O11>0,P11>0),Q11/(O11*P11*0.001),0)/O4","v":0},{"$f":"+Q35+P35*P38","v":54.14602769631724},null,null,null,"Rth","Q"]
[null,null,null,null,null,"HS1",6.471196682144971E-2,15.468729799643645,null,null,"HS",{"$f":"+G37","v":6.471196682144971E-2},{"$f":"M36+(L38/M38)","v":29.479516429498183},null,"HS",{"$f":"+U37","v":1.0060975609756098},{"$f":"Q36+P38/Q38","v":52.066712894212849},null,null,"HS1",1.0060975609756098,1]
[null,null,null,null,null,"HS2",40120,2.5000000000000001E-5,null,null,"ENV",null,{"$f":"+D2","v":25},null,"ENV",null,{"$f":"+V2","v":50},null,null,"HS2",1525.4490490675551,7.479272152569851E-4]
[null,null,null,null,null,null,6.471196682144971E-2,15.468729799643645,null,null,null,{"$f":"SUM(L31:L35)","v":0.19349749601440619},null,null,null,{"$f":"SUM(P31:P35)","v":12.00609756097561},null,null,null,null,1.0060975609756098,1]
[null,null,null,null,null,null,null,null,null,null,"Heat",{"$f":"+E17+F4*G4*H4*(1-J4/100)/1000","v":69.292429280971874},{"$f":"H37","v":15.468729799643645},null,null,{"$f":"W17+O4*P4*Q4*(1-S4/100)/1000","v":2.0667128942128481},{"$f":"V37","v":1}]

{"sheet":"TM_D","index":7,"n_rows":38,"n_cols":34,"rows_kept":38,"cut":false,"hidden":true,"merged":[]}
[null,null,"快速热分析工具(TAM)",null,null,null,null,null,null,null,"等效Rth","Tj","Tj","等效Rth"]
[null,null,"环境温度",25,"  (C)","n","If","Vf","Rth","效率",{"$f":"+L37","v":0.34089755805847771},{"$f":"+M35+L37*L38","v":77.91174363561079},{"$f":"+Q35+P37*P38","v":102.79658279092392},{"$f":"+P37","v":4.5554836496717037},"n","If","Vf","Rth","效率",null,"环境温度",50,"( C)"]
[null,null,null,null,null,null,"(mA)","(V)","(C/W)","%",null,null,null,null,null,"(mA)","(V)","(C/W)","%",null,null,"材料",null,null,null,null,"光源个数","电流(mA)",null,null,"总功率",null,"帮助档案："]
[null,null,"光源","Everlight-XI3030-2S-R80-1W",null,142,200,6.600000000000013,15,50,null,null,null,null,9,240,6.7299755673715929,15,50,null,"光源","Everlight-XI3030-2S-R80-1W",null,null,null,null,1,800,null,null,{"$f":"+I6","v":187.44000000000034},"W"]
[null,null,null,null,null,"k","面积","厚度","总功率",null,null,null,null,null,"k","面积","厚度","總功率",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"线上帮助：","IJR website"]
[null,null,null,"材料",null,"(W/mK)","(mm2)","(mm)",{"$f":"H4*G4*F4/1000","v":187.44000000000034},null,null,null,null,null,"(W/mK)","(mm2)","(mm)",{"$f":"Q4*P4*O4/1000","v":14.536747225522641},null,null,null,null,null,null,null,null,"封装形式：",null,null,"PCB 面积",{"$f":"260*61","v":15860},"mm2","Email: ","sales@ichijouriki.com"]
[null,null,"焊点","SAC-G",null,58,3.3349999999999995,0.15,null,null,null,null,null,null,380,3.3349999999999995,7.0000000000000007E-2,null,null,null,"焊点","Cu_pure-G"]
[null,null,"焊点","SAC-G",null,58,1.1499999999999999,0.15,null,null,null,null,null,null,58,1.1499999999999999,7.0000000000000007E-2,null,null,null,"焊点","SAC-G",null,null,null,null,null,null,null,null,"LED",1,"LED"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(a*b)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"焊點",2,"焊点"]
[null,null,"PCB","Ideal-MCPCB-G",null,33.729999999999997,111.69014084507042,1.2,null,null,null,null,null,null,0.2,500,0.11600000000000001,null,null,null,"PCB","Ideal-FR4-G",null,null,null,null,null,null,null,null,"PCB",3,"PCB"]
[null,null,"热介材料","Eporite-TIM3101",null,6,111.69014084507042,0.5,null,null,null,null,null,null,2.56,500,0.2,null,null,null,"热介材料","Eporite-TIM1101",null,null,null,null,null,null,null,null,"熱介材料",4,"热介材料"]
[null,null,null,null,null,"Thermal",null,"Fin",null,null,null,null,null,null,"Thermal",null,"Fin",null,null,null,null,null,null,null,null,null,null,null,null,null,"散熱器",5,"散热器"]
[null,null,null,null,null,"h","k","n","b","t",null,null,null,null,"h","k","n","b","t",null,null,null,null,null,null,null,null,null,null,null,"鰭片",6,"鳍片"]
[null,null,null,"材料","几何尺寸","(W/m2K)","(W/mK)",null,"(mm)","(mm)",null,null,null,null,"(W/m2K)","(W/mK)",null,"(mm)","(mm)",null,null,"材料","几何尺寸",null,null,null,null,null,null,null,"環境溫度",7,"环境温度"]
[null,null,"散热器1","Al-6063-Extruded","PCC-Flooding-180W",8,170,4,1,630,null,null,null,null,12,164,80,2,22,null,"散热器1","Al-G","G-S22x22x6-1.5W"]
[null,null,"散热器2",null,null,0,0,0,5,50,null,null,null,null,12,164,0,1E-3,100,null,"散热器2","Al-G","G-P100x100x10-7W"]
[null,null,"Driver",null,0,"(W)",null,"Block",null,null,null,null,null,null,null,null,"Block",null,null,null,"Driver",null,0]
[null,null,null,null,"(W)",null,null,"L","l","delta",null,null,null,null,null,null,"L","l","delta",null,null,null,"(W)"]
[null,null,null,null,null,null,null,"(mm)","(mm)","(mm)",null,null,null,null,null,null,"(mm)","(mm)","(mm)"]
[null,null,null,null,null,null,null,310,90,1,null,null,null,null,null,null,22,6,2]
[null,null,null,null,null,null,null,50,10,3,null,null,null,null,null,null,100,1E-3,10]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Temp1",null,null,null,"Temp1"]
[null,null,null,null,null,"solder","1/r","1/r",null,null,null,"Rth1",{"$f":"+M31+L31*L38","v":77.91174363561079},null,null,"Rth1",{"$f":"+Q31+P31*P38","v":102.79658279092392},null,null,null,"solder","1/r","1/r"]
[null,null,null,null,null,null,{"$f":"+F7*G7/1000/H7","v":1.2895333333333334},{"$f":"+F8*G8/1000/H8","v":0.44466666666666665},null,null,"LS",{"$f":"I4/F4","v":0.10563380281690141},{"$f":"+M32+L32*L38","v":68.01174363561077},null,"LS",{"$f":"R4/O4","v":1.6666666666666667},{"$f":"+Q32+P32*P38","v":90.682626769655059},null,null,null,null,{"$f":"+O7*P7/1000/Q7","v":18.104285714285709},{"$f":"+O8*P8/1000/Q8","v":0.95285714285714274}]
[null,null,null,null,null,"sum 1/r",{"$f":"+G31+H31","v":1.7342},{"$f":"IF(G32>0,1/G32,0)","v":0.57663475954330523},null,null,"SOLDER",{"$f":"+H32/F4","v":4.060808165797924E-3},{"$f":"+M33+L33*L38","v":67.63116469431219},null,"SOLDER",{"$f":"+W32/O4","v":5.8304181242711996E-3},{"$f":"+Q33+P33*P38","v":90.640249112409236},null,null,null,"sum 1/r",{"$f":"+V31+W31","v":19.05714285714285},{"$f":"IF(V32>0,1/V32,0)","v":5.2473763118440798E-2}]
[null,null,null,null,null,null,null,null,null,null,"PCB",{"$f":"IF(AND(F10>0,G10>0),H10/(F10*G10*0.001),0)/F4","v":2.2431675919109884E-3},{"$f":"+M34+L34*L38","v":67.42093502759829},null,"PCB",{"$f":"IF(AND(O10>0,P10>0),Q10/(O10*P10*0.001),0)/O4","v":0.12888888888888889},{"$f":"+Q34+P34*P38","v":89.703436513431114}]
[null,null,null,null,null,null,"Rth","Q",null,null,"TIM",{"$f":"IF(AND(F11>0,G11>0),H11/(F11*G11*0.001),0)/F4","v":5.2543085329970571E-3},{"$f":"+M35+L35*L38","v":66.928501231885804},null,"TIM",{"$f":"IF(AND(O11>0,P11>0),Q11/(O11*P11*0.001),0)/O4","v":1.7361111111111112E-2},{"$f":"+Q35+P35*P38","v":89.577249471542899},null,null,null,"Rth","Q"]
[null,null,null,null,null,"HS1",0.22370547095087034,4.4707715806698536,null,null,"HS",{"$f":"+G37","v":0.22370547095087034},{"$f":"M36+(L38/M38)","v":45.962824494370196},null,"HS",{"$f":"+U37","v":2.7367365648807662},{"$f":"Q36+P38/Q38","v":69.685625638284478},null,null,"HS1",4.0735446406338109,0.24922238319039436]
[null,null,null,null,null,"HS2",40120,2.5000000000000001E-5,null,null,"ENV",null,{"$f":"+D2","v":25},null,"ENV",null,{"$f":"+V2","v":50},null,null,"HS2",8.3394308943089435,0.12]
[null,null,null,null,null,null,0.22370547095087034,4.4707715806698536,null,null,null,{"$f":"SUM(L31:L35)","v":0.34089755805847771},null,null,null,{"$f":"SUM(P31:P35)","v":4.5554836496717037},null,null,null,null,2.7367365648807662,0.36922238319039435]
[null,null,null,null,null,null,null,null,null,null,"Heat",{"$f":"+E17+F4*G4*H4*(1-J4/100)/1000","v":93.720000000000184},{"$f":"H37","v":4.4707715806698536},null,null,{"$f":"W17+O4*P4*Q4*(1-S4/100)/1000","v":7.2683736127613203},{"$f":"V37","v":0.36922238319039435}]

{"sheet":"Sheet2","index":8,"n_rows":40,"n_cols":33,"rows_kept":40,"cut":false,"hidden":true,"merged":[]}
[null,null,"快速熱分析工具(TAM)",null,null,null,null,null,null,null,"等效Rth","Tj","Tj","等效Rth"]
[null,null,"環境溫度",25,"( C)","n","If","Vf","Rth","效率",{"$f":"+L37","v":5.0210641533556526},{"$f":"+M35+L37*L38","v":106.77946792668075},{"$f":"+Q35+P37*P38","v":243.80371146162818},{"$f":"+P37","v":3.8726714067229335},"n","If","Vf","Rth","效率",null,"環境溫度",50,"( C)"]
[null,null,null,null,null,null,"(mA)","(V)","(C/W)","%",null,null,null,null,null,"(mA)","(V)","(C/W)","%",null,null,"材料",null,null,null,null,"光源個數","電流(mA)",null,null,"總功率",null,"幫助檔案："]
[null,null,"光源","Everlight-XI3030",null,{"$f":"+AA4","v":44},{"$f":"+AB4","v":80},5.8101947391864197,15,50,null,null,null,null,40,200,6.6712894212848006,11,50,null,"光源","光源",null,null,null,null,44,80,null,null,{"$f":"+I6","v":20.451885481936198},"W","線上幫助："]
[null,null,null,null,null,"k","面積","厚度","總功率",null,null,null,null,null,"k","面積","厚度"]
[null,null,null,"材料",null,"(W/mK)","(mm2)","(mm)",{"$f":"H4*G4*F4/1000","v":20.451885481936198},null,null,null,null,null,"(W/mK)","(mm2)","(mm)",null,null,null,null,null,null,null,null,null,"封裝形式：",null,null,"PCB 面積",{"$f":"800*30","v":24000},"mm2"]
[null,null,"焊點","SAC-G",null,58,3.4154999999999998,0.15,null,null,null,null,null,null,58,3.2915000000000001,7.0000000000000007E-2,null,null,null,"焊點","General-SAC",null,null,null,null,null,null,null,null,null,"溫度"]
[null,null,"焊點","SAC-G",null,58,1.1499999999999999,0.15,null,null,null,null,null,null,10,1.0895999999999999,7.0000000000000007E-2,null,null,null,"焊點","General-AgSP",null,null,null,null,null,null,null,null,"LED",106.77946792668075]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"(a*b)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"焊點",103.2933510831689]
[null,null,"PCB","Ideal-FR4-G",null,0.2,{"$f":"IF(AE6>0,AE6/F4,H20*J15/F4)","v":545.4545454545455},1.2,null,null,null,null,null,null,33.729999999999997,500,0.11600000000000001,null,null,null,"PCB","General-Ideal-MCPCB",null,null,null,null,null,null,null,null,"PCB",103.16169964779672]
[null,null,"熱介材料","CS-DSTape",null,1.5,5.25732,0.5,null,null,null,null,null,null,2.56,500,0.2,null,null,null,"熱介材料","Eporite-TIM1101",null,null,null,null,null,null,null,null,"熱介材料",100.6052139625547]
[null,null,null,null,null,"Thermal",null,"Fin",null,null,null,null,null,null,"Thermal",null,"Fin",null,null,null,null,null,null,null,null,null,null,null,null,null,"散熱器",85.869709334882756]
[null,null,null,null,null,"h","k","n","b","t",null,null,null,null,"h","k","n","b","t",null,null,null,null,null,null,null,null,null,null,null,"鰭片",55.434353395738384]
[null,null,null,"材料","幾何尺寸","(W/m2K)","(W/mK)",null,"(mm)","(mm)",null,null,null,null,"(W/m2K)","(W/mK)",null,"(mm)","(mm)",null,null,"材料","幾何尺寸",null,null,null,null,null,null,null,"環境溫度",25]
[null,null,"散熱器1","Al-6063-Extruded","G-S1000x42x29",8,170,0,2,1000,null,null,null,null,12,58,24,5,50,null,"散熱器1","General-SAC","TS-Dot1"]
[null,null,"散熱器2",null,null,0,0,0,5,50,null,null,null,null,0,0,15,2,90,null,"散熱器2","散热器2"]
[null,null,"Driver",null,0,"(W)",null,"Block",null,null,null,null,null,null,null,null,"Block",null,null,null,"Driver","Driver",0,"(W)"]
[null,null,null,null,"(W)",null,null,"L","l","delta",null,null,null,null,null,null,"L","l","delta",null,null,null,"(W)"]
[null,null,null,null,null,null,null,"(mm)","(mm)","(mm)",null,null,null,null,null,null,"(mm)","(mm)","(mm)"]
[null,null,null,null,null,null,null,42,29,0.7,null,null,null,null,null,null,50,10,20]
[null,null,null,null,null,null,null,50,10,3,null,null,null,null,null,null,59,38,10]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"G-GC230x203-x3-13W"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Temp1",null,null,null,"Temp1"]
[null,null,null,null,null,"solder","1/r","1/r",null,null,null,"Rth1",{"$f":"+M31+L31*L38","v":106.77946792668075},null,null,"Rth1",{"$f":"+Q31+P31*P38","v":243.80371146162818},null,null,null,"solder","1/r","1/r"]
[null,null,null,null,null,null,{"$f":"+F7*G7/1000/H7","v":1.3206599999999999},{"$f":"+F8*G8/1000/H8","v":0.44466666666666665},null,null,"LS",{"$f":"I4/F4","v":0.34090909090909088},{"$f":"+M32+L32*L38","v":103.2933510831689},null,"LS",{"$f":"R4/O4","v":0.27500000000000002},{"$f":"+Q32+P32*P38","v":236.46529309821491},null,null,null,null,{"$f":"+O7*P7/1000/Q7","v":2.7272428571428571},{"$f":"+O8*P8/1000/Q8","v":0.15565714285714283}]
[null,null,null,null,null,"sum 1/r",{"$f":"+G31+H31","v":1.7653266666666667},{"$f":"IF(G32>0,1/G32,0)","v":0.56646739602490948},null,null,"SOLDER",{"$f":"+H32/F4","v":1.2874259000566124E-2},{"$f":"+M33+L33*L38","v":103.16169964779672},null,"SOLDER",{"$f":"+W32/O4","v":8.671823511047904E-3},{"$f":"+Q33+P33*P38","v":236.23388412040489},null,null,null,"sum 1/r",{"$f":"+V31+W31","v":2.8828999999999998},{"$f":"IF(V32>0,1/V32,0)","v":0.34687294044191613}]
[null,null,null,null,null,null,null,null,null,null,"PCB",{"$f":"IF(AND(F10>0,G10>0),H10/(F10*G10*0.001),0)/F4","v":0.24999999999999992},{"$f":"+M34+L34*L38","v":100.6052139625547},null,"PCB",{"$f":"IF(AND(O10>0,P10>0),Q10/(O10*P10*0.001),0)/O4","v":1.7195375037058996E-4},{"$f":"+Q34+P34*P38","v":236.2292955074617}]
[null,null,null,null,null,null,"Rth","Q",null,null,"TIM",{"$f":"IF(AND(F11>0,G11>0),H11/(F11*G11*0.001),0)/F4","v":1.4409922880398331},{"$f":"+M35+L35*L38","v":85.869709334882756},null,"TIM",{"$f":"IF(AND(O11>0,P11>0),Q11/(O11*P11*0.001),0)/O4","v":3.90625E-3},{"$f":"+Q35+P35*P38","v":236.12505661025412},null,null,null,"Rth","Q"]
[null,null,null,null,null,"HS1",2.9762885154061625,0.33600000000000002,null,null,"HS",{"$f":"+G37","v":2.9762885154061625},{"$f":"M36+(L38/M38)","v":55.434353395738384},null,"HS",{"$f":"+U37","v":3.5849213794615151},{"$f":"Q36+P38/Q38","v":140.46086431049685},null,null,"HS1",3.5849213794615151,0.29499118639354777]
[null,null,null,null,null,"HS2",40120,2.5000000000000001E-5,null,null,"ENV",null,{"$f":"+D2","v":25},null,"ENV",null,{"$f":"+V2","v":50},null,null,"HS2",1525.4490490675551,7.479272152569851E-4]
[null,null,null,null,null,null,2.9762885154061625,0.33600000000000002,null,null,null,{"$f":"SUM(L31:L35)","v":5.0210641533556526},null,null,null,{"$f":"SUM(P31:P35)","v":3.8726714067229335},null,null,null,null,3.5849213794615151,0.29499118639354777]
[null,null,null,null,null,null,null,null,null,null,"Heat",{"$f":"+E17+F4*G4*H4*(1-J4/100)/1000","v":10.225942740968099},{"$f":"H37","v":0.33600000000000002},null,null,{"$f":"W17+O4*P4*Q4*(1-S4/100)/1000","v":26.685157685139202},{"$f":"V37","v":0.29499118639354777}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"G-GC230x203-x3-4W"]

{"sheet":"TM_S-bp","index":9,"n_rows":38,"n_cols":24,"rows_kept":38,"cut":false,"hidden":true,"merged":[]}
["快速熱分析工具(TAM)",null,null,null,null,null,null,null,null,null,"等效Rth","Tj","Tj","等效Rth"]
[null,null,"環境溫度",25,"( C)","n","If","Vf","Rth","效率",{"$f":"+L37","v":48.500576278790611},{"$f":"+M35+L37*L38","v":80.252651891885222},{"$f":"+Q35+P37*P38","v":243.80371146162818},{"$f":"+P37","v":3.8726714067229335},"n","If","Vf","Rth","效率",null,"環境溫度",50,"( C)"]
[null,null,null,"材料",null,null,"(mA)","(V)","(C/W)","%",null,null,null,null,null,"(mA)","(V)","(C/W)","%",null,null,"材料"]
[null,null,"光源","Everlight-XI5050",null,1,100,18.115452430929277,10,50,null,null,null,null,40,200,6.6712894212848006,11,50,null,"光源","光源"]
[null,null,null,null,null,"k","面積","厚度","總功率",null,null,null,null,null,"k","面積","厚度"]
[null,null,null,null,null,"(W/mK)","(mm2)","(mm)",{"$f":"H4*G4*F4/1000","v":1.8115452430929277},null,null,null,null,null,"(W/mK)","(mm2)","(mm)"]
[null,null,"焊點","General-SAC",null,58,8.5399999999999991,0.1,null,null,null,null,null,null,58,3.2915000000000001,7.0000000000000007E-2,null,null,null,"焊點","General-SAC"]
[null,null,"焊點","General-SAC",null,58,2.145,0.1,null,null,null,null,null,null,10,1.0895999999999999,7.0000000000000007E-2,null,null,null,"焊點","General-AgSP"]
[null,null,null,null,null,null,"A=PCB面積/光源個數 或 COB面積*1.2",null,null,null,null,null,null,null,null,"(a*b)"]
[null,null,"PCB","General-Ideal-FR4",null,0.2,{"$f":"100/F4","v":100},0.5,null,null,null,null,null,null,33.729999999999997,{"$f":"20*300/12","v":500},0.11600000000000001,null,null,null,"PCB","General-Ideal-MCPCB"]
[null,null,"熱介材料","Eporite-TIM3101",null,6,{"$f":"G10","v":100},0.5,null,null,null,null,null,null,2.56,500,0.2,null,null,null,"熱介材料","Eporite-TIM1101"]
[null,null,null,null,null,"Thermal",null,"Fin",null,null,null,null,null,null,"Thermal",null,"Fin"]
[null,null,null,null,null,"h","k","n","b","t",null,null,null,null,"h","k","n","b","t"]
[null,null,null,"材料","幾何尺寸","(W/m2K)","(W/mK)",null,"(mm)","(mm)",null,null,null,null,"(W/m2K)","(W/mK)",null,"(mm)","(mm)",null,null,"材料","幾何尺寸"]
[null,null,"散熱器1","Extruded-Al-A6063","G-P100x100x10",8,170,0,1E-3,100,null,null,null,null,12,58,24,5,50,null,"散熱器1","General-SAC","TS-Dot1"]
[null,null,"散熱器2",null,null,0,0,0,5,50,null,null,null,null,0,0,15,2,90,null,"散熱器2","散热器2"]
[null,null,"Driver",null,0,"(W)",null,"Block",null,null,null,null,null,null,null,null,"Block",null,null,null,"Driver","Driver",0,"(W)"]
[null,null,null,null,"(W)",null,null,"L","l","delta",null,null,null,null,null,null,"L","l","delta",null,null,null,"(W)"]
[null,null,null,null,null,null,null,"(mm)","(mm)","(mm)",null,null,null,null,null,null,"(mm)","(mm)","(mm)"]
[null,null,null,null,null,null,null,100,1E-3,10,null,null,null,null,null,null,50,10,20]
[null,null,null,null,null,null,null,50,10,3,null,null,null,null,null,null,59,38,10]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Temp1",null,null,null,"Temp1"]
[null,null,null,null,null,"solder","1/r","1/r",null,null,null,"Rth1",{"$f":"+M31+L31*L38","v":80.252651891885208},null,null,"Rth1",{"$f":"+Q31+P31*P38","v":243.80371146162818},null,null,null,"solder","1/r","1/r"]
[null,null,null,null,null,null,{"$f":"+F7*G7/1000/H7","v":4.9531999999999989},{"$f":"+F8*G8/1000/H8","v":1.2440999999999998},null,null,"LS",{"$f":"I4/F4","v":10},{"$f":"+M32+L32*L38","v":71.194925676420567},null,"LS",{"$f":"R4/O4","v":0.27500000000000002},{"$f":"+Q32+P32*P38","v":236.46529309821491},null,null,null,null,{"$f":"+O7*P7/1000/Q7","v":2.7272428571428571},{"$f":"+O8*P8/1000/Q8","v":0.15565714285714283}]
[null,null,null,null,null,"sum 1/r",{"$f":"+G31+H31","v":6.1972999999999985},{"$f":"IF(G32>0,1/G32,0)","v":0.16136059251609575},null,null,"SOLDER",{"$f":"+H32/F4","v":0.16136059251609575},{"$f":"+M33+L33*L38","v":71.048769669522969},null,"SOLDER",{"$f":"+W32/O4","v":8.671823511047904E-3},{"$f":"+Q33+P33*P38","v":236.23388412040489},null,null,null,"sum 1/r",{"$f":"+V31+W31","v":2.8828999999999998},{"$f":"IF(V32>0,1/V32,0)","v":0.34687294044191613}]
[null,null,null,null,null,null,null,null,null,null,"PCB",{"$f":"IF(AND(F10>0,G10>0),H10/(F10*G10*0.001),0)/F4","v":25},{"$f":"+M34+L34*L38","v":48.404454130861374},null,"PCB",{"$f":"IF(AND(O10>0,P10>0),Q10/(O10*P10*0.001),0)/O4","v":1.7195375037058996E-4},{"$f":"+Q34+P34*P38","v":236.2292955074617}]
[null,null,null,null,null,null,"Rth","Q",null,null,"TIM",{"$f":"IF(AND(F11>0,G11>0),H11/(F11*G11*0.001),0)/F4","v":0.83333333333333337},{"$f":"+M35+L35*L38","v":47.64964361290599},null,"TIM",{"$f":"IF(AND(O11>0,P11>0),Q11/(O11*P11*0.001),0)/O4","v":3.90625E-3},{"$f":"+Q35+P35*P38","v":236.12505661025412},null,null,null,"Rth","Q"]
[null,null,null,null,null,"HS1",12.505882352941176,0.08,null,null,"HS",{"$f":"+G37","v":12.505882352941176},{"$f":"M36+(L38/M38)","v":36.322157769330801},null,"HS",{"$f":"+U37","v":3.5849213794615151},{"$f":"Q36+P38/Q38","v":140.46086431049685},null,null,"HS1",3.5849213794615151,0.29499118639354777]
[null,null,null,null,null,"HS2",40120,2.5000000000000001E-5,null,null,"ENV",null,{"$f":"+D2","v":25},null,"ENV",null,{"$f":"+V2","v":50},null,null,"HS2",1525.4490490675551,7.479272152569851E-4]
[null,null,null,null,null,null,12.505882352941176,0.08,null,null,null,{"$f":"SUM(L31:L35)","v":48.500576278790611},null,null,null,{"$f":"SUM(P31:P35)","v":3.8726714067229335},null,null,null,null,3.5849213794615151,0.29499118639354777]
[null,null,null,null,null,null,null,null,null,null,"Heat",{"$f":"+E17+F4*G4*H4*(1-J4/100)/1000","v":0.90577262154646387},{"$f":"H37","v":0.08},null,null,{"$f":"W17+O4*P4*Q4*(1-S4/100)/1000","v":26.685157685139202},{"$f":"V37","v":0.29499118639354777}]

{"sheet":"LSI","index":10,"n_rows":22,"n_cols":29,"rows_kept":22,"cut":false,"hidden":true,"merged":[]}
["Light source information Import"]
["光源數據輸入"]
["光源数据输入",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"drawing"]
[null,null,null,"Supplier",null,"Nichia",null,"PAD1",null,null,null,null,null,null,"Efficacy",null,null,null,"Vf-If"]
[null,null,null,"Type",null,"SMD_3030",null,"x","(mm)",1.45,null,null,null,null,"If",65,null,null,"If",65,null,null,null,"Eff-If",null,null,null,"Vf-If"]
[null,null,null,"Name",null,"NF2L757GT",null,"y","(mm)",2.27,null,null,null,null,"Vf",2.75,null,null,"Lm",33.700000000000003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,{"$f":"+O9","v":65},{"$f":"$O$11*EXP(-$O$12*X7)","v":159.44055944055944},null,0,{"$f":"+S9","v":65},{"$f":"+$S$12*AB7^$S$11","v":2.75}]
[null,null,null,"If","(mA)",180,null,"PAD2",null,null,null,null,null,null,"Eff-If","Lm","Eff",null,null,"Vf",null,null,1,{"$f":"+$X$7+W8*($X$17-$X$7)/10","v":82.5},157.43209111615232,null,1,{"$f":"+$AB$7+AA8*($AB$17-$AB$7)/10","v":82.5},{"$f":"+$S$12*AB8^$S$11","v":2.8107925048732043}]
[null,null,null,"Vf","(V)",3,null,"x","(mm)",0.48,null,null,null,"If",65,28.5,{"$f":"+P9/O9/T9*1000","v":159.44055944055944},"If",65,2.75,null,null,2,{"$f":"+$X$7+W9*($X$17-$X$7)/10","v":100},155.44892341176495,null,2,{"$f":"+$AB$7+AA9*($AB$17-$AB$7)/10","v":100},2.8608237730510924]
[null,null,null,null,null,null,null,"y","(mm)",2.27,null,null,null,null,240,{"$f":"+P9/0.9*3.3","v":104.49999999999999},{"$f":"+P10/O10/T10*1000","v":140.45698924731181},null,240,3.1,null,null,3,117.5,153.49073761618567,null,3,117.5,2.9034512563711909]
[null,null,null,"Rth","(C/W)",11,null,null,null,null,null,null,null,"A",{"$f":"Q9/(EXP(-O12*O9))","v":167.12752371538375},null,null,"D",{"$f":"LOG10(T9/S12)/LOG10(S9)","v":9.1713721086241512E-2},null,null,null,4,135,151.55721903299906,null,4,135,2.9406578792848359]
[null,null,null,"Efficiency","(%)",50,null,null,null,null,null,null,null,"B",{"$f":"-LN(Q9/Q10)/(O9-O10)","v":7.2439925216408012E-4},null,null,"C",{"$f":"10^S14","v":1.8752693864979155},null,null,null,5,152.5,149.64805693001173,null,5,152.5,2.9737158344340204]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"+LOG10(S9)/LOG10(S10)","v":0.76166069837532258},null,null,null,6,170,147.76294448931529,null,6,170,3.0034916863355745]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(S13*LOG10(T10)-LOG10(T9))/(-1+S13)","v":0.27306366388559788},null,null,null,7,187.5,145.90157875797792,null,7,187.5,3.0306031379952878]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8,205,144.06366059935758,null,8,205,3.0555065055161621]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,222.5,142.24889464502823,null,9,222.5,3.0785487429547991]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,{"$f":"+O10","v":240},140.45698924731181,null,10,{"$f":"+S10","v":240},3.1000000000000005]
[]
[]
[]
[null,null,"Supplier","Type","LS","Code","If","Vf","Rth","Efficiency","A","B","C","D","PAD1_X","PAD1_Y","PAD2_X","PAD2_Y"]
[null,null,{"$f":"+F4","v":"Nichia"},{"$f":"+F5","v":"SMD_3030"},{"$f":"+F6","v":"NF2L757GT"},{"$f":"+C22 & \"-\" & E22","v":"Nichia-NF2L757GT"},{"$f":"+F8","v":180},{"$f":"+F9","v":3},{"$f":"+F11","v":11},{"$f":"+F12","v":50},{"$f":"+O11","v":167.12752371538375},{"$f":"+O12","v":7.2439925216408012E-4},{"$f":"+S12","v":1.8752693864979155},{"$f":"+S11","v":9.1713721086241512E-2},{"$f":"+J5","v":1.45},{"$f":"+J6","v":2.27},{"$f":"+J9","v":0.48},{"$f":"+J10","v":2.27}]

{"sheet":"Sheet1","index":11,"n_rows":14,"n_cols":11,"rows_kept":14,"cut":false,"hidden":true,"merged":[]}
[null,null,null,null,null,{"$f":"COUNT(F4:F210)","v":11}]
[null,"Supplier/App","Product","Code","Code","n","b","t","L","l","delta"]
[null,null,null,null,null,null,"(mm)","(mm)","(mm)","(mm)","(mm)"]
[null,"G","Plate","P100x100x10",{"$f":"B4& \"-\"&D4","v":"G-P100x100x10"},0,1E-3,100,100,1E-3,10]
[null,"G","Plate","P500x500x20","G-P500x500x20",0,1E-3,500,500,1E-3,20]
[null,"G","HS","S22x22x6","G-S22x22x6",8,2,22,22,6,2]
[null,"G","HS","S200x50x30",{"$f":"B7& \"-\"&D7","v":"G-S200x50x30"},11,2.5,200,50,30,2.5]
[null,"G","HS","S290x80x40",{"$f":"B8& \"-\"&D8","v":"G-S290x80x40"},20,2,80,290,40,4]
[null,"G","HS","S1000x42x29",{"$f":"B9& \"-\"&D9","v":"G-S1000x42x29"},2,2,1000,42,29,0.7]
[null,"G","HS","S430x410x120",{"$f":"B10& \"-\"&D10","v":"G-S430x410x120"},32,1,410,430,120,1]
[null,"G","HS","S510x430x220",{"$f":"B11& \"-\"&D11","v":"G-S510x430x220"},42,1,430,510,220,1]
[null,"G","HS","C83x24x47","G-C83x24x47",24,1,47,110,24,1]
[null,"G","HS","C160x45x220",{"$f":"B13& \"-\"&D13","v":"G-C160x45x220"},28,2,220,220,45,2]
[null,"G","HS","C240x150x45",{"$f":"B14& \"-\"&D14","v":"G-C240x150x45"},72,2,240,470,45,2]

{"sheet":"DB_LSI","index":12,"n_rows":100,"n_cols":18,"rows_kept":100,"cut":false,"hidden":true,"merged":[]}
[]
[null,"Supplier","Type","LS","Code","If","Vf","Rth","Efficiency","A","B","C","D","PAD1_X","PAD1_Y","PAD2_X","PAD2_Y"]
[null,null,null,null,null,"(mA)","(V)","(C/W)","%"]
[null,"Nichia","SMD_3030","NF2L757GT","Nichia-NF2L757GT",180,3,11,50,167.12752371538375,7.2439925216408012E-4,1.8752693864979155,9.1713721086241512E-2,1.45,2.27,0.48,2.27]
[null,"Everlight","SMD_3030","XI3030","Everlight-XI3030",240,3,15,50,154.05231178061342,2.1491486131170784E-3,2.8381666235803458,0.16349873228287934,1.4850000000000001,2.2999999999999998,0.5,2.2999999999999998]
[null,"Everlight","SMD_5050","XI5050","Everlight-XI5050",240,16.666666666666668,10,50,195.43780086978597,2.1709804676264214E-3,10.21477108224294,0.12441027330704636,2.8,3.05,3.3,0.65]
[null,"Cree","SMD","XPG","Cree-Xlamp-XPG",350,2.9,4,50,134.32982009251393,3.1761625011315133E-4,1.8331826594403235,7.8296749120179129E-2,1.3,3.3,1,3.3]
[null,"Cree","SMD_3535","XP-L-HI","Cree-Xlamp-XP-L-HI",3000,2.95,2.2000000000000002,50,95.782894368512132,8.324128757384058E-5,1.2702625568967592,0.12112068560754218,3.3,1.3,3.3,1]
[null,"Cree","XPE","XPE_white_CRI80","Cree-XPE_white_CRI80",1000,3,9,45,103.2577332690194,5.7925120947445636E-4,1.4151337393923846,0.13109018629395552,1,3.3,1.3,3.3]
[null,"Cree","XPE","XPE_Green","Cree-XPE_Green",1000,3,15,45,116.36251488129457,8.4468744090182828E-4,1.501874320228713,0.13438333501237165,1,3.3,1.3,3.3]
[null,"Cree","XPE","XPE_Red","Cree-XPE_Red",700,3,8,52.631578947368432,127.20741324259491,8.8776087441571824E-4,0.73964860087696516,0.16105235934580178,1,3.3,1.3,3.3]
[null,"Citizen","COB","CLU056","Citizen-CLU056",5750,52,0.22,50,204.04511379501633,1.4233916383861637E-4,19.083351929411489,0.12987022090383932,38,19,38,19]
[null,"Citizen","COB","CLU048","Citizen-CLU048",4140,52,0.17,50,140.74309549779119,1.0510228801743046E-4,17.281679231122062,0.14906221083998047,28,14,28,14]
[null,"Cree","COB","CXA3590","Cree-CXA3590",3600,41.6,1,50,164.21126008415609,1.7372515698323604E-4,8.7067545710242911,0.19099529016149183,34.85,34.85,0.01,0.01]
[null,"Cree","COB","CXA3070","Cree-CXA3070",2800,38.5,0.7,50,184.631801856397,2.4371277191085768E-4,11.310779325791117,0.16224708072143595,27.35,27.35,0.01,0.01]
[null,"Cree","COB","CXA2540","Cree-CXA2540",2100,36.200000000000003,0.7,50,154.51893134276594,2.8441204061070479E-4,15.283727873656654,0.1231275645122638,27.35,27.35,0.01,0.01]
[null,"Sunpu","COB","G17-4829MX","Sunpu-G17-4829MX",1200,36,0.8,50,224.68949406601095,6.6542308018147632E-4,4.4140524323168684,0.31396374801627003,19,19,0.01,0.01]
[null,"Sunpu","COB","G17-4427MX","Sunpu-G17-4427MX",300,145,0.8,50,259.49672322124536,3.2170948047792491E-3,23.144482275765348,0.32860347854487471,19,19,0.01,0.01]
[null,"Everlight",2835,"2835HE","Everlight-2835HE-R80-0.2W",180,2.85,30,50,238.13067512781188,3.4567993250851259E-3,1.5762484862390547,0.13332573806735865,2,2,0.9,2]
[null,"Everlight",2835,"3020S","Everlight-3020S-R80-0.2W",75,3.25,50,50,164.78688253789844,3.805501026135724E-3,2.2632136667493152,7.2870225359476404E-2,1.5,1.4,0.8,1.4]
[null,"Everlight",2835,2835,"Everlight-2835-R80-0.2W",60,3.05,50,50,193.81762851394103,4.9438943191897579E-3,1.6002063560672404,0.14939450444010538,2,2,0.9,2]
[null,"Everlight",0.2,"5630D-HE","Everlight-5630D-HE-R80-0.2W",180,2.75,21,50,247.87128289555559,2.5122912293715741E-3,1.8666749653011472,0.10137062331808608,3.37,1.6,1.1200000000000001,1.6]
[null,"Everlight",0.5,"5630B","Everlight-5630B-R75-0.5W",180,3.15,21,50,140.7155231728776,2.1643295522130535E-3,1.8622943019731084,0.10424534654742823,2.1,1.5,2.4,1]
[null,"Everlight",0.5,"2835HV","Everlight-2835HV-R80-0.5W",40,18.5,21,50,180.60501344640085,1.2451294787258252E-2,14.432422576016751,6.65749938865806E-2,2,2,0.9,2]
[null,"Everlight",0.5,2835,"Everlight-2835-R80-0.5W",180,3.2,21,50,214.53353500207498,2.8787412359062921E-3,1.0051721562142633,0.24024927950727973,2,2,0.9,2]
[null,"Everlight",0.5,"5630B","Everlight-5630B-R75-0.5W",180,3.15,21,50,140.7155231728776,2.1643295522130535E-3,1.8622943019731084,0.10424534654742823,2.4,1,2.1,1.5]
[null,"Everlight",1,"A22_HV","Everlight-A22_HV-R80-1W",150,15,9,50,168.77320759734118,1.4046819076947259E-3,9.9904745141336342,9.148098448280613E-2,3.8,3.9,2.8,3.2]
[null,"Everlight",0.5,"A22","Everlight-A22-R80-0.5W",150,3.4,9,50,179.03132262252862,3.9546767157768396E-3,0.62033934912019673,0.32109515669071836,3.8,3.9,2.8,3.2]
[null,"Everlight",4,"XI5050","Everlight-XI5050-R80-4W",240,15,10,50,177.55960412246441,1.5983412361847856E-3,10.519414774132258,0.11723262681851156,2.8,3.05,0.65,3.3]
[null,"Everlight",8,"XI9595","Everlight-XI9595-R80-8W",200,44,5,50,142.4149612624565,4.0942693549235958E-4,24.738449094269019,8.5914628706592985E-2,8,6,8,2.46]
[null,"Everlight",1,"ELSWF_3535","Everlight-ELSWF_3535-R80-1W",1000,44,5,50,163.63687211973684,7.1915048432353624E-4,0.51843298744717359,0.27851190850908936,1.3,3.1,1.36,3.1]
[null,"Everlight",1,2835,"Everlight-2835-R80-1W",200,6.1999999999999993,17,50,200.12457933395208,1.951727503675432E-3,3.5147843987944749,0.11487630690556702,2,2,0.9,2]
[null,"Everlight",1,"XI3535","Everlight-XI3535-R80-1W",350,3.4000000000000004,15,50,117.63080751744027,6.3872859206714485E-4,1.9866887237220587,8.4020368356844038E-2,2.0550000000000002,2.5,0.42,2.5]
[null,"Everlight",1,"XI3030-2S","Everlight-XI3030-2S-R80-1W",240,3.4000000000000004,15,50,135.59415214232291,1.2756893779619998E-3,3.7446936597701761,0.10696411634030985,1.45,2.2999999999999998,0.5,2.2999999999999998]
[null,"Everlight",1,"XI3535-6V","Everlight-XI3535-6V-R80-1W",240,6.5,15,50,136.08320453823666,1.0547718675002126E-3,3.3600270075791916,0.12765855428051795,2.0550000000000002,2.66,0.42,2.66]
[null,"Everlight",25,"XUAN1919","Everlight-XUAN1919-R80-25W",1440,36,0.46,50,139.08798397877808,1.8193500476652646E-4,18.472806708783725,9.816560785130056E-2,19,19,1E-3,1E-3]
[null,"Everlight",8,"XUAN1313","Everlight-XUAN1313-R80-8W",480,36,1.5,50,156.20457576113739,7.6252293264194855E-4,23.827357668289107,7.137605489439959E-2,13.5,13.5,1E-3,1E-3]
[null,"Everlight",15,"JU2024","Everlight-JU2024-R80-15W",550,36,2.4,50,143.67403956861145,4.0183500219699727E-4,14.200426567748174,0.11917350427999052,20,24,1E-3,1E-3]
[null,"Everlight",10,"JU1215","Everlight-JU1215-R80-10W",800,18,2.4,50,131.89777499890491,2.7381205865617921E-4,10.729627254606225,8.0684094928577615E-2,15,12,1E-3,1E-3]
[null,"Citizen",2,"CLU025","Citizen-CLU025-R80-2W",540,8.9,5.3,50,155.54390657845559,5.6372178817026743E-4,7.0145580709486293,4.2523333296084515E-2,13.5,13.5,1E-3,1E-3]
[null,"Citizen",11,"CLU701","Citizen-CLU701-R80-11W",460,52,1.6,50,128.48463223805018,2.7619537739472335E-4,16.819652834286092,0.1060416374103251,13.5,13.5,1E-3,1E-3]
[null,"Citizen",12,"CLU028","Citizen-CLU028-R97-12W",920,34.6,0.91,45,135.48596880370314,5.6905974479109828E-4,11.879491848706431,0.1816210072078068,13.5,13.5,1E-3,1E-3]
[null,"Citizen",12,"CLU038","Citizen-CLU038-R97-25W",1840,34.6,0.51,45,123.10433602074791,1.8362236141981206E-4,18.232721624881222,0.10276337525959714,19,19,1E-3,1E-3]
[null,"Citizen",36,"CLU038","Citizen-CLU038-R80-36W",2300,52,0.42,50,177.03998930340114,1.9258042061132767E-4,14.330586856897364,0.13334617501995275,19,19,1E-3,1E-3]
[null,"Citizen",84,"CLU046","Citizen-CLU046-R80-84W",4140,104,0.26,50,175.44481885906794,1.4958041503284388E-4,7.2727483175628436,0.26617877817342017,28,28,1E-3,1E-3]
[null,"Citizen",56,"CLU048","Citizen-CLU048-R97-56W",2760,52,0.25,45,129.98190778799722,1.2411695131699915E-4,22.691974959062545,0.11723262681851147,28,28,1E-3,1E-3]
[null,"Citizen",84,"CLU048","Citizen-CLU048-R80-84W",4140,52,0.17,50,161.68550161420794,8.6956991246754775E-5,25.469672451937235,0.10128333583718117,28,28,1E-3,1E-3]
[null,"Citizen",168,"CLU058","Citizen-CLU058-R80-168W",4140,52,0.1,50,165.51112134131296,9.3877947598235457E-5,44.350261171391445,0.11950709445608843,38,38,1E-3,1E-3]
[null,"Citizen",168,"CLU056","Citizen-CLU056-R80-168W",4140,104,0.15,50,177.58796643311689,1.5131420231352419E-4,14.04942077750945,0.27074406067124884,38,38,1E-3,1E-3]
[null,"Citizen",242,"CLU550","Citizen-CLU550-R80-242W",4680,104,0.1,50,178.03679406488905,1.1400515770144411E-4,17.497633524531015,0.22961907577223184,38,38,1E-3,1E-3]
[null,"Cree",0.3,"ML-B","Cree-ML-B-R80-0.3W",175,3.5,25,50,119.29788859895085,3.660212921409927E-3,1.7471907449806934,0.14511852893452218,3.1999999999999997,2.3000000000000003,0.9,3.2,-13]
[null,"Cree",0.3,"ML-C","Cree-ML-C-R80-0.3W",350,3.5,13,50,166.78709535833167,3.6012415558544981E-3,1.6066495904959086,0.14695457135040971,3.1999999999999997,2.3000000000000003,0.9,3.2,-13]
[null,"Cree",0.3,"ML-E","Cree-ML-E-R80-0.3W",500,3.2,11,50,109.63179671936787,1.1227820342111069E-3,1.5976530382780427,0.13749249216457463,3.1999999999999997,2.3000000000000003,0.9,3.2,-13]
[null,"Cree",1,"MX-3","Cree-MX-3-R80-1W",500,3.7,11,50,145.47349691980253,1.7428331965218969E-3,2.0625061990061377,9.5779202562789267E-2,3.5,3.9,1.1000000000000001,3.9,-2.7]
[null,"Cree",1,"MX-3S","Cree-MX-3S-R80-1W",175,3.2,11,50,121.08126895181795,3.4784704271230934E-3,5.4001954725508758,0.14438990933517484,3.5,3.9,1.1000000000000001,3.9,-13]
[null,"Cree",1,"MX-6","Cree-MX-6-R80-1W",1000,3.7,5,50,117.30368059385626,6.1686930987512722E-4,1.5144736503759657,0.14277713096799954,3.5,3.9,1.1000000000000001,3.9,-3.3]
[null,"Cree",1,"XB-D","Cree-XB-D-R80-1W",1000,2.9,6.5,50,139.55009830167327,6.2032522428671834E-4,1.6618323000110049,9.5048873636340514E-2,0.92,2.29,0.66,2.29,-2.5]
[null,"Cree",3,"XB-H","Cree-XB-H-R80-3W",1500,2.9,4,50,154.24053150688081,3.7987163791576713E-4,1.4246449785835515,0.10849937045432302,0.92,2.29,0.72,2.29,-2.2000000000000002]
[null,"Cree",4,"XHP35","Cree-XHP35-R80-4W",1050,11.3,1.8,50,162.87064977521391,4.5148185458129494E-4,6.8859428779101188,8.4555532330077149E-2,1.3,3.3,1,3.3,-8]
[null,"Cree",0.2,"XH-B","Cree-XH-B-R80-0.2W",175,3.1,45,50,142.46136557006588,3.1515574423663793E-3,1.9052953811654427,0.11774464988037769,1.7,3,0.8,3,-2]
[null,"Cree",0.2,"XH-G","Cree-XH-G-R80-0.2W",350,2.9,20,50,171.71647273299439,2.0675426846904826E-3,1.2678848744130515,0.18516859120823781,1.7,3,0.8,3,-1.2]
[null,"Cree",3,"XM-L","Cree-XM-L-R80-3W",350,2.9,2.5,50,124.72284075422507,2.0071749749409236E-4,1.5149171169728843,9.9121057075553118E-2,2.78,4.78,1,4.78,-2.1]
[null,"Cree",3,"XM-L-HV","Cree-XM-L-HV-R80-3W",125,46,3.5,50,135.83688628055594,3.2029031776320506E-3,36.458009603562495,6.2765441041929326E-2,2.78,4.78,1,4.78,-35]
[null,"Cree",5,"XM-L2","Cree-XM-L2-R80-5W",3000,3.3,2.5,50,154.26430495500517,2.4089973797155592E-4,1.4731056982298281,0.10073851464309617,2.78,4.78,1,4.78,-1.6]
[null,"Cree",5,"XP-C","Cree-XP-C-R80-1W",500,3.3,12,50,125.91245462396083,1.2625988828494866E-3,0.73446338575675707,0.25124321237737501,1.3,3.3,1,3.3,-4]
[null,"Cree",3,"XP-E","Cree-XP-E-R80-3W",1000,3.1,9,50,124.56657316931965,6.2094551114569622E-4,1.4151337393923846,0.13109018629395552,1.3,3.3,1,3.3,-3]
[null,"Cree",3,"XP-E-HEW","Cree-XP-E-HEW-R80-3W",1000,3.1,6,50,144.26110011366504,4.3680161905578738E-4,1.9193366754305703,7.6244066309575198E-2,1.3,3.3,1,3.3,-3]
[null,"Cree",3,"XP-E2","Cree-XP-E2-R80-3W",1000,3.1,9,50,153.77859065903229,7.0394689332982938E-4,1.8281359021850576,7.8767358693836984E-2,1.3,3.3,1,3.3,-2.2999999999999998]
[null,"Cree",5,"XP-G","Cree-XP-G-R80-5W",1500,3.1,9,50,143.85525713222148,3.3189084942647539E-4,1.8331826594403235,7.8296749120179129E-2,1.3,3.3,1,3.3,-3.9]
[null,"Cree",5,"XP-G2","Cree-XP-G2-R80-5W",1500,3.1,4,50,157.85650519841306,3.0574224278029529E-4,1.8587718123981072,6.9939934900425188E-2,1.3,3.3,1,3.3,-1.8]
[null,"Cree",6,"XP-G3","Cree-XP-G3-R80-6W",2000,3.1,3,50,151.90793075821759,2.7029670837171296E-4,1.7379046342615594,7.4429946260140448E-2,1.3,3.3,1,3.3,-1.3]
[null,"Cree",9,"XP-L","Cree-XP-L-R80-9W",3000,3.1,2.2000000000000002,50,180.83610502845988,1.8758092286988982E-4,1.3482828908517208,0.11255203126252779,1.3,3.3,1,3.3,-2]
[null,"Cree",1,"XQ-A","Cree-XQ-A-R80-1W",300,3,20,50,123.73892489451104,2.0119971335558129E-3,1.8770475520584773,9.0863999147355115E-2,0.65,1.6,1.65,1.6,-2.8]
[null,"Cree",1,"XQ-B","Cree-XQ-B-R80-1W",300,3,17,50,127.26871224793076,1.634780656587705E-3,2.1870091751836527,7.2130404035574802E-2,0.65,1.6,1.65,1.6,-32]
[null,"Cree",2,"XQ-D","Cree-XQ-D-R80-2W",700,3,7.5,50,113.49935482288811,5.9487701008512073E-4,1.8403762726575437,8.9012976252220363E-2,0.65,1.6,1.65,1.6,-3]
[null,"Cree",3,"XQ-E","Cree-XQ-E-R80-3W",1000,3,6,50,127.30330562269751,5.38949286981237E-4,1.8497007209092386,7.6765451501625961E-2,0.65,1.6,1.65,1.6,-2.2999999999999998]
[null,"Cree",2,"XR-C","Cree-XR-C-R75-2W",500,3.5,12,50,102.19576459055627,1.1752711204549653E-3,2.0688601717295967,8.4804248286778169E-2,2.75,3.7,0.6,5,-4]
[null,"Cree",2,"XR-C","Cree-XR-C-R75-2W",1000,3.5,12,50,111.28233582774058,7.1714484549883595E-4,2.0070158775173668,8.4888897586513301E-2,2.75,3.7,0.6,5,-4]
[null,"Cree",9,"MC-E","Cree-MC-E-R80-9W",1000,3.5,3,50,92.866681170008277,6.5919508905697025E-4,1.420111915106764,0.13326653086346432,4,2.84,0.6,1.1599999999999999,-4]
[null,"Cree",7,"MHB-A","Cree-MHB-A-R80-7W",175,36,5.5,50,172.4513327519457,3.1589930667966556E-3,25.612011464843761,7.8737464867807389E-2,2.78,4.78,1,3.6,-16]
[null,"Cree",13,"MHD-E","Cree-MHD-E-R80-13W",350,36,3.2,50,157.90026717987507,1.209743394276824E-3,18.403897526074438,0.12820207436163417,3.9,6.76,1.4,6.76,-15]
[null,"Cree",19,"MHD-G","Cree-MHD-G-R80-19W",500,36,2.6,50,153.58628514530417,9.9762971228916633E-4,17.767003344045225,0.12243666212260436,3.9,6.76,1.4,6.76,-17]
[null,"Cree",15,"MK-R","Cree-MK-R-R80-15W",1250,18,1.7,50,140.258587473391,2.4157942664669788E-4,7.3490747186301633,7.0982861046271717E-2,3.9,6.76,1.4,6.76,-8]
[null,"Cree",25,"MT-G","Cree-MT-G-R77-25W",700,36,1.5,50,115.70552803742851,9.6359319908606523E-4,22.6255884934649,7.5179537942039992E-2,6,8.9,1.9,8.9,-27]
[null,"Cree",18.5,"MT-G2","Cree-MT-G2-R80-18.5W",500,36,1.5,50,133.38267106854875,1.0106382601621554E-3,22.624857156063015,7.9147184960419281E-2,6,8.9,1.9,8.9,-26]
[null,"Cree",19,"XHP50","Cree-XHP50-R80-19W",1500,12,1.2,50,147.8380251299026,2.9213324225581445E-4,6.4735400982712061,8.7714375532820341E-2,2.78,4.78,1,4.78,-9]
[null,"Cree",32,"XHP70","Cree-XHP70-R80-32W",2400,12,0.9,50,156.31010304870679,2.3663531924826851E-4,5.47978910398027,0.10780328953451537,3.9,6.76,1.4,6.76,-8.5]
[null,"Cree",13,"XM-L","Cree-XM-L-R80-13W",1000,12,2.5,50,111.43098138818692,7.9138483284990993E-4,5.7165152520697609,0.11932325256384455,2.78,4.78,1,4.78,-12]
[null,"Cree",13,"XM-L2","Cree-XM-L2-R80-13W",1000,12,2.5,50,131.95619190637879,5.6250924201824766E-4,7.3125436087402171,7.8767358693837289E-2,2.78,4.78,1,4.78,-10]
[null,"Cree",20,"CXA1310","Cree-CXA1310-R80-20W",525,36,2,50,131.97722216015995,9.0021721681935341E-4,21.805895981116247,8.3675459219869699E-2,13.35,13.35,1E-3,1E-3]
[null,"Cree",33,"CXA1520","Cree-CXA1520-R80-33W",900,35,2,50,138.3382064527998,5.5966218681151628E-4,22.218560755983063,7.3121272433757392E-2,15.85,15.85,1E-3,1E-3]
[null,"Cree",78,"CXA1850","Cree-CXA1850-R80-78W",2100,35,0.6,50,131.0117200953799,1.9466928010973482E-4,18.973710409772121,8.3724224172498737E-2,17.850000000000001,17.850000000000001,1E-3,1E-3]
[null,"Cree",130,"CXA2590","Cree-CXA2590-R80-130W",1800,69,0.3,50,137.66808872845903,2.3835507797061387E-4,45.455640072201966,5.7819322390426781E-2,23.85,23.85,1E-3,1E-3]
[null,"Cree",150,"CXA3090","Cree-CXA3090-R80-150W",1800,72,0.6,50,161.252984641984,3.3230089298641122E-4,19.87840843331848,0.19099529016149047,34.85,34.85,1E-3,1E-3]
[null,"Cree",24,"CXB1310","Cree-CXB1310-R80-24W",350,33,3,50,142.02544692087901,4.9386544008833016E-4,25.778208838561579,4.2161294534676777E-2,13.35,13.35,1E-3,1E-3]
[null,"Cree",49,"CXB1520","Cree-CXB1520-R80-49W",1400,33,2.6,50,156.16336017211844,2.6228585713824662E-4,24.99709182500861,4.4692773215250982E-2,15.85,15.85,1E-3,1E-3]
[null,"Cree",53,"CXB1830","Cree-CXB1830-R80-53W",1400,35,1,50,188.947335825317,3.6367119972133597E-4,16.285030523405194,0.1144571711278001,17.850000000000001,17.850000000000001,1E-3,1E-3]
[null,"Cree",79,"CXB2540","Cree-CXB2540-R80-79W",2100,34.799999999999997,0.7,50,189.99772612070259,3.006632673225795E-4,18.269092456454246,9.2017802117218106E-2,23.85,23.85,1E-3,1E-3]
[null,"Cree",107,"CXB3070","Cree-CXB3070-R80-107W",2800,34.799999999999997,0.4,50,243.82490379513166,2.9619795122770462E-4,14.66073352290271,0.11899241244527235,27.35,27.35,1E-3,1E-3]
[null,"Cree",137,"CXB3590","Cree-CXB3590-R80-137W",1800,72,0.3,50,211.58104936884345,3.5077823688751318E-4,36.649651093991196,9.5240464428685487E-2,34.85,34.85,1E-3,1E-3]

{"sheet":"DB_METAL","index":13,"n_rows":13,"n_cols":6,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
[null,null,null,null,null,{"$f":"COUNT(F4:F19)","v":10}]
[null,"Supplier","Type","Mat","Code","k"]
[null,null,null,null,null,"(W/mK)"]
[null,"G","solder paste","AgSP",{"$f":"D4& \"-\"&B4","v":"AgSP-G"},10]
[null,"G","SAC ","SAC",{"$f":"D5& \"-\"&B5","v":"SAC-G"},58]
[null,"G","Cu","Cu_pure",{"$f":"D6& \"-\"&B6","v":"Cu_pure-G"},380]
[null,"Extruded","Al","Al-6063",{"$f":"D7& \"-\"&B7","v":"Al-6063-Extruded"},170]
[null,"G","Al","Al",{"$f":"D8& \"-\"&B8","v":"Al-G"},164]
[null,"General","solder paste","AgSP",{"$f":"B9& \"-\"&D9","v":"General-AgSP"},10]
[null,"General","SAC ","SAC","General-SAC",58]
[null,"General","Al","Al","General-Al",164]
[null,"General","Cu","Cu_pure","General-Cu_pure",380]
[null,"Extruded","Al","Al-A6063","Extruded-Al-A6063",170]

{"sheet":"DB_PCB","index":14,"n_rows":13,"n_cols":6,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
[null,null,null,null,null,{"$f":"COUNT(F4:F18)","v":10}]
[null,"Supplier","Type","Mat","Code","k"]
[null,null,null,null,null,"(W/mK)"]
[null,"G","MCPCB","Ideal-MCPCB",{"$f":"D4& \"-\"&B4","v":"Ideal-MCPCB-G"},33.729999999999997]
[null,"G","FR4","Ideal-FR4",{"$f":"D5& \"-\"&B5","v":"Ideal-FR4-G"},0.2]
[null,"G","Ceramic","99Ceramic(AlO)-Ideal",{"$f":"D6& \"-\"&B6","v":"99Ceramic(AlO)-Ideal-G"},31]
[null,"G","Ceramic","95Ceramic(AlO)-Ideal",{"$f":"D7& \"-\"&B7","v":"95Ceramic(AlO)-Ideal-G"},22]
[null,"G","Ceramic","Ceramic(AlN)",{"$f":"D8& \"-\"&B8","v":"Ceramic(AlN)-G"},180]
[null,"General","MCPCB","Ideal-MCPCB",{"$f":"B9& \"-\"&D9","v":"General-Ideal-MCPCB"},33.729999999999997]
[null,"General","FR4","Ideal-FR4","General-Ideal-FR4",0.2]
[null,"General","Ceramic","99Ceramic(AlO)-Ideal","General-99Ceramic(AlO)-Ideal",31]
[null,"General","Ceramic","95Ceramic(AlO)-Ideal","General-95Ceramic(AlO)-Ideal",22]
[null,"General","Ceramic","Ceramic(AlN)","General-Ceramic(AlN)",180]

{"sheet":"DB_TIM","index":15,"n_rows":8,"n_cols":6,"rows_kept":8,"cut":false,"hidden":true,"merged":[]}
[null,null,null,null,null,{"$f":"COUNT(F4:F19)","v":5}]
[null,"Supplier","Type","Mat","Code","k"]
[null,null,null,null,null,"(W/mK)"]
[null,"CS","TIM","DSTape",{"$f":"B4& \"-\"&D4","v":"CS-DSTape"},1.5]
[null,"Eporite","TIM","TIM1101","Eporite-TIM1101",2.56]
[null,"Eporite","TIM","TIM2001",{"$f":"B6& \"-\"&D6","v":"Eporite-TIM2001"},2]
[null,"Eporite","TIM","TIM3101",{"$f":"B7& \"-\"&D7","v":"Eporite-TIM3101"},6]
[null,"Eporite","TIM","TIM0001",{"$f":"B8& \"-\"&D8","v":"Eporite-TIM0001"},2]

{"sheet":"DB_DRV","index":16,"n_rows":5,"n_cols":8,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
[null,null,null,null,null,{"$f":"COUNT(F4:F170)","v":2}]
[null,"Supplier","Type","Mat","Code","Q"]
[null,null,null,null,null,"W"]
[null,"DRV","Driver","Test1",{"$f":"B4& \"-\"&D4","v":"DRV-Test1"},2,null,"輸入：散熱功率＝總功率＊（1-效率）"]
[null,"DRV","Driver","Test0",{"$f":"B5& \"-\"&D5","v":"DRV-Test0"},0]

{"sheet":"DB_HS","index":17,"n_rows":35,"n_cols":12,"rows_kept":35,"cut":false,"hidden":true,"merged":[]}
[null,null,null,null,null,{"$f":"COUNT(F4:F167)","v":32}]
[null,"Supplier/App","Product","Code","Code","n","b","t","L","l","delta"]
[null,null,null,null,null,null,"(mm)","(mm)","(mm)","(mm)","(mm)"]
[null,"G","Plate","P100x100x10","G-P100x100x10-7W",0,1E-3,100,100,1E-3,10]
[null,"G","Plate","P500x500x20","G-P500x500x20-115W",0,1E-3,500,500,1E-3,20]
[null,"G","HS","S22x22x6","G-S22x22x6-1.5W",8,2,22,22,6,2]
[null,"G","HS","S200x50x30","G-S200x50x30-70W",11,2.5,200,50,30,2.5]
[null,"G","HS","S290x80x40","G-S290x80x40-75W",20,2,80,290,40,4]
[null,"G","HS","S1000x42x29","G-S1000x42x29-80W",2,2,1000,42,29,0.7]
[null,"G","HS","C83x24x47","G-C83x24x47-28W",24,1,47,110,24,1]
[null,"G","HS","C160x45x220","G-C160x45x220-200W",28,2,220,220,45,2]
[null,"G","HS","C240x150x45","G-C240x150x45-500W",72,2,240,470,45,2]
[null,"G","HS","S430x410x120",{"$f":"B13& \"-\"&D13&\"-\"&L13&\"W\"","v":"G-S430x410x120-400W"},32,1,410,430,120,1,400]
[null,"G","HS","S510x430x220","G-S510x430x220-1000W",42,1,430,510,220,1,1000]
[null,"PCC","HS","Sport","PCC-Sport-400W",32,2,430,416,100,1]
[null,"PCC","HS","Sport","PCC-Sport-500W",32,1,410,430,120,1]
[null,"PCC","HS","Sport","PCC-Sport-1000W",42,1,430,510,220,1]
[null,"PCC","HS","Project","PCC-Project-180W",32,1,200,550,23,1]
[null,"PCC","HS","Project","PCC-Project-600W",32,1,320,300,170,1]
[null,"PCC","HS","Hproject","PCC-Hproject-600W",32,1,300,300,175,1]
[null,"PCC","HS","Hproject","PCC-Hproject-400W",32,1,250,250,175,1]
[null,"PCC","HS","HProject","PCC-HProject-300W",32,1,250,250,160,1]
[null,"PCC","HS","Flooding","PCC-Flooding-200W",4,1,730,310,90,1]
[null,"PCC","HS","Flooding","PCC-Flooding-180W",4,1,630,310,90,1]
[null,"PCC","HS","Flooding","PCC-Flooding-120W",4,1,540,310,90,1]
[null,"PCC","HS","ProjectS","PCC-ProjectS-140W",27,1,190,250,25,1]
[null,"PCC","HS","ProjectS","PCC-ProjectS-120W",27,1,170,225,25,1]
[null,"PCC","HS","ProjectS","PCC-ProjectS-100W",27,1,150,215,25,1]
[null,"PCC","HS","Factory","PCC-Factory-150W",24,20,150,470,30,1]
[null,"PCC","HS","Factory","PCC-Factory-130W",24,20,130,470,30,1]
[null,"PCC","HS","Factory","PCC-Factory-100W",24,20,120,470,30,1]
[null,"PCC","HS","Street","PCC-Street-150W",12,1,590,215,25,1]
[null,"PCC","HS","Tunnel","PCC-Tunnel-180W",52,1,360,600,45,1]
[null,"PCC","HS","Tunnel","PCC-Tunnel-120W",26,1,300,430,45,1]
[null,"PCC","HS","Tunnel","PCC-Tunnel-90W",26,1,300,340,45,1]

{"sheet":"HS_D","index":18,"n_rows":17,"n_cols":25,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["HS Calculation","Heat transfer coefficient",null,null,null,"Geometry"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"e","Rj",1,2,3,"Q","Tf"]
[null,"Fin","bottom","Fin Tip","k","Number of Fins","Length","Width","Height","Fin width","Block","heatsink bottom area",null,null,null,null,"case1",{"$f":"G11","v":{"$error":"#REF!"}},{"$f":"O11","v":{"$error":"#REF!"}},{"$f":"+$F$7*SQRT($B$7*$E$7*C11*B11)","v":{"$error":"#REF!"}},{"$f":"TANH(SQRT($B$7*B11/($E$7*C11))*$I$7)","v":{"$error":"#REF!"}},{"$f":"$C$7*($L$7-$F$7*C11)","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"+W3/(T3*U3+V3)+#REF!","v":{"$error":"#REF!"}}]
[null,"(W/m2K)",null,null,"(W/mK)",null,"mm","mm","mm","mm",null,"mm2",null,null,null,null,"case2",{"$f":"J13","v":{"$error":"#REF!"}},{"$f":"Y13","v":{"$error":"#REF!"}},{"$f":"+$F$7*SQRT($B$7*$E$7*C13*B13)","v":{"$error":"#REF!"}},{"$f":"(TANH(D13)+E13)/(1+E13*TANH(D13))","v":{"$error":"#REF!"}},{"$f":"$C$7*($L$7-$F$7*C13)","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"+W4/(T4*U4+V4)+#REF!","v":{"$error":"#REF!"}}]
[null,"hf","hb","he","k","n/a","L","t","l","b","delta","A",null,null,null,null,"case3",{"$f":"J15","v":{"$error":"#REF!"}},{"$f":"Y15","v":{"$error":"#REF!"}},{"$f":"+$F$7*SQRT($B$7*$E$7*C15*B15)","v":{"$error":"#REF!"}},{"$f":"TANH(SQRT($B$7*B15/($E$7*C15))*$I$7)","v":{"$error":"#REF!"}},{"$f":"$C$7*($L$7-$F$7*C15)","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"+W5/(T5*U5+V5)+#REF!","v":{"$error":"#REF!"}}]
[null,{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"B6","v":{"$error":"#REF!"}},{"$f":"C6","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"H6*G6","v":{"$error":"#REF!"}},null,null,null,null,"case4",{"$f":"J17","v":{"$error":"#REF!"}},{"$f":"Y17","v":{"$error":"#REF!"}},{"$f":"+$F$7*SQRT($B$7*$E$7*C17*B17)","v":{"$error":"#REF!"}},{"$f":"(TANH(D17)+E17)/(1+E17*TANH(D17))","v":{"$error":"#REF!"}},{"$f":"$C$7*($L$7-$F$7*C17)","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}},{"$f":"+W6/(T6*U6+V6)+#REF!","v":{"$error":"#REF!"}}]
[null,{"$f":"+B6","v":{"$error":"#REF!"}},{"$f":"+C6","v":{"$error":"#REF!"}},{"$f":"+D6","v":{"$error":"#REF!"}},{"$f":"+E6","v":{"$error":"#REF!"}},{"$f":"+F6","v":{"$error":"#REF!"}},{"$f":"+G6*0.001","v":{"$error":"#REF!"}},{"$f":"+H6*0.001","v":{"$error":"#REF!"}},{"$f":"+I6*0.001","v":{"$error":"#REF!"}},{"$f":"+J6*0.001","v":{"$error":"#REF!"}},{"$f":"+K6*0.001","v":{"$error":"#REF!"}},{"$f":"+G7*H7","v":{"$error":"#REF!"}}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AVERAGE(S3:S6)","v":{"$error":"#REF!"}},{"$f":"AVERAGE(T3:T6)","v":{"$error":"#REF!"}},{"$f":"AVERAGE(U3:U6)","v":{"$error":"#REF!"}},{"$f":"AVERAGE(V3:V6)","v":{"$error":"#REF!"}},null,{"$f":"AVERAGE(X3:X6)","v":{"$error":"#REF!"}}]
[]
["case 1","p","a","m",null,null,"e","v","D","S","Bi","H",null,"yida","R",null,null,null,null,null,null,{"$f":"+T8*U8+V8","v":{"$error":"#REF!"}}]
[null,{"$f":"2*H7","v":{"$error":"#REF!"}},{"$f":"+J7*H7","v":{"$error":"#REF!"}},{"$f":"SQRT(B6*B11/(E6*C11))","v":{"$error":"#REF!"}},{"$f":"F7*SQRT(B7*C11*E7*B11)/(C7*L7)","v":{"$error":"#REF!"}},{"$f":"TANH(SQRT(B7*B11/(E7*C11))*I7)","v":{"$error":"#REF!"}},{"$f":"E11*F11+1-F7*C11/(L7)","v":{"$error":"#REF!"}},{"$f":"J7*H7*G7","v":{"$error":"#REF!"}},{"$f":"F7/(L7) *SQRT(H11*H7)","v":{"$error":"#REF!"}},{"$f":"I7*SQRT( (H7)/H11)","v":{"$error":"#REF!"}},{"$f":"2*B7/E7*SQRT(H11/(H7))","v":{"$error":"#REF!"}},{"$f":"D6/B6","v":{"$error":"#REF!"}},{"$f":"2*I11*J11/L11+1-I11/J11","v":{"$error":"#REF!"}},{"$f":"G11/M11","v":{"$error":"#REF!"}},{"$f":"(1/L7)*(1/(G11*C7)+K7/E7)","v":{"$error":"#REF!"}}]
["case 2","p","a","M","N",null,null,null,null,"e","v","D","S","Bi","H","Hb","He","E","I","J","F","K",null,"yida","Rj"]
[null,{"$f":"2*$H$7","v":{"$error":"#REF!"}},{"$f":"+$J$7*$H$7","v":{"$error":"#REF!"}},{"$f":"SQRT(($B$7*B13)/($E$7*C13))*$I$7","v":{"$error":"#REF!"}},{"$f":"+($D$7*$I$7)/(D13*$E$7)","v":{"$error":"#REF!"}},{"$f":"SQRT($B$7*B13/($E$7*C13))","v":{"$error":"#REF!"}},{"$f":"$F$7*SQRT($B$7*$E$7*C13*B13)/($C$7*$L$7)","v":{"$error":"#REF!"}},{"$f":"TANH(F13*$I$7)+$D$7/(F13*$E$7)","v":{"$error":"#REF!"}},{"$f":"1+$D$7/(F13*$E$7)*TANH(F13*$I$7)","v":{"$error":"#REF!"}},{"$f":"+G13*H13/I13+1-$F$7*C13/$L$7","v":{"$error":"#REF!"}},{"$f":"$J$7*$H$7*$G$7","v":{"$error":"#REF!"}},{"$f":"$F$7/($L$7) *SQRT(K13*$H$7)","v":{"$error":"#REF!"}},{"$f":"$I$7*SQRT( ($H$7)/K13)","v":{"$error":"#REF!"}},{"$f":"2*$B$7/$E$7*SQRT(K13/($H$7))","v":{"$error":"#REF!"}},{"$f":"$D$7/$B$7","v":{"$error":"#REF!"}},{"$f":"+$C$7/$B$7","v":{"$error":"#REF!"}},{"$f":"+$D$7/$B$7","v":{"$error":"#REF!"}},{"$f":"2*L13/(SQRT(N13)*P13)","v":{"$error":"#REF!"}},{"$f":"+Q13/P13*L13","v":{"$error":"#REF!"}},{"$f":"0.5*SQRT(N13)*Q13","v":{"$error":"#REF!"}},{"$f":"SQRT(N13)","v":{"$error":"#REF!"}},{"$f":"SQRT(K13/$H$7^3)","v":{"$error":"#REF!"}},{"$f":"2*L13*M13/O13+1-(1+$D$7/$C$7)*(L13/M13)","v":{"$error":"#REF!"}},{"$f":"+J13/W13","v":{"$error":"#REF!"}},{"$f":"(1/$L$7)*(1/(J13*$C$7)+$K$7/$E$7)","v":{"$error":"#REF!"}}]
["case 3","p","a","M","N",null,null,null,null,"e","v","D","S","Bi","H","Hb","He","E","I","J","F",null,null,"yida","Rj"]
[null,{"$f":"2*($H$7+$J$7)","v":{"$error":"#REF!"}},{"$f":"+$J$7*$H$7","v":{"$error":"#REF!"}},{"$f":"SQRT(($B$7*B15)/($E$7*C15))*$I$7","v":{"$error":"#REF!"}},{"$f":"+($D$7*$I$7)/(D15*$E$7)","v":{"$error":"#REF!"}},{"$f":"SQRT($B$7*B15/($E$7*C15))","v":{"$error":"#REF!"}},null,{"$f":"+F7*SQRT(B7*E7*C15*B15)/(C7*L7)","v":{"$error":"#REF!"}},{"$f":"TANH(SQRT(B7*B15/(E7*C15))*I7)","v":{"$error":"#REF!"}},{"$f":"+H15*I15+1-F7*C15/L7","v":{"$error":"#REF!"}},{"$f":"$J$7*$H$7*$G$7","v":{"$error":"#REF!"}},{"$f":"$F$7/($L$7) *SQRT(K15*$H$7)","v":{"$error":"#REF!"}},{"$f":"$I$7*SQRT( ($H$7)/K15)","v":{"$error":"#REF!"}},{"$f":"2*$B$7/$E$7*SQRT(K15/($H$7))","v":{"$error":"#REF!"}},{"$f":"$D$7/$B$7","v":{"$error":"#REF!"}},{"$f":"+$C$7/$B$7","v":{"$error":"#REF!"}},{"$f":"+$D$7/$B$7","v":{"$error":"#REF!"}},{"$f":"2*L15/(SQRT(N15)*P15)","v":{"$error":"#REF!"}},{"$f":"+Q15/P15*L15","v":{"$error":"#REF!"}},{"$f":"0.5*SQRT(N15)*Q15","v":{"$error":"#REF!"}},{"$f":"SQRT(N15)","v":{"$error":"#REF!"}},{"$f":"SQRT(K15/$H$7^3)","v":{"$error":"#REF!"}},{"$f":"2*L15*V15/O15+2*L15*M15/O15+1-L15/M15","v":{"$error":"#REF!"}},{"$f":"+J15/W15","v":{"$error":"#REF!"}},{"$f":"(1/$L$7)*(1/(J15*$C$7)+$K$7/$E$7)","v":{"$error":"#REF!"}}]
["case 4","p","a","M","N",null,null,null,null,"e","v","D","S","Bi","H","Hb","He","E","I","J","F",null,null,"yida","Rj"]
[null,{"$f":"2*($H$7+$J$7)","v":{"$error":"#REF!"}},{"$f":"+$J$7*$H$7","v":{"$error":"#REF!"}},{"$f":"SQRT(($B$7*B17)/($E$7*C17))*$I$7","v":{"$error":"#REF!"}},{"$f":"+($D$7*$I$7)/(D17*$E$7)","v":{"$error":"#REF!"}},{"$f":"SQRT($B$7*B17/($E$7*C17))","v":{"$error":"#REF!"}},{"$f":"$F$7*SQRT($B$7*$E$7*C17*B17)/($C$7*$L$7)","v":{"$error":"#REF!"}},{"$f":"TANH(F17*$I$7)+$D$7/(F17*$E$7)","v":{"$error":"#REF!"}},{"$f":"1+$D$7/(F17*$E$7)*TANH(F17*$I$7)","v":{"$error":"#REF!"}},{"$f":"+G17*H17/I17+1-$F$7*C17/$L$7","v":{"$error":"#REF!"}},{"$f":"$J$7*$H$7*$G$7","v":{"$error":"#REF!"}},{"$f":"$F$7/($L$7) *SQRT(K17*$H$7)","v":{"$error":"#REF!"}},{"$f":"$I$7*SQRT( ($H$7)/K17)","v":{"$error":"#REF!"}},{"$f":"2*$B$7/$E$7*SQRT(K17/($H$7))","v":{"$error":"#REF!"}},{"$f":"$D$7/$B$7","v":{"$error":"#REF!"}},{"$f":"+$C$7/$B$7","v":{"$error":"#REF!"}},{"$f":"+$D$7/$B$7","v":{"$error":"#REF!"}},{"$f":"2*L17/(SQRT(N17)*P17)","v":{"$error":"#REF!"}},{"$f":"+Q17/P17*L17","v":{"$error":"#REF!"}},{"$f":"0.5*SQRT(N17)*Q17","v":{"$error":"#REF!"}},{"$f":"SQRT(N17)","v":{"$error":"#REF!"}},{"$f":"SQRT(K17/$H$7^3)","v":{"$error":"#REF!"}},{"$f":"2*L17*M17/O17+1-(1+$D$7/$C$7)*(L17/M17)+2*L17*V17/O17","v":{"$error":"#REF!"}},{"$f":"+J17/W17","v":{"$error":"#REF!"}},{"$f":"(1/$L$7)*(1/(J17*$C$7)+$K$7/$E$7)","v":{"$error":"#REF!"}}]